diff -u -r ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.8 ./wpa_supplicant/doc/docbook/wpa_supplicant.8
--- ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.8	2020-03-10 21:49:08.458858646 +0100
+++ ./wpa_supplicant/doc/docbook/wpa_supplicant.8	2020-03-10 21:52:22.866338065 +0100
@@ -348,7 +348,7 @@
 .RS
 
 .nf
-wpa_supplicant -B -c/etc/wpa_supplicant.conf -iwlan0
+wpa_supplicant -B -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0
 .fi
 .RE
 .PP
@@ -361,7 +361,7 @@
 .RS
 
 .nf
-wpa_supplicant -c/etc/wpa_supplicant.conf -iwlan0 -d
+wpa_supplicant -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0 -d
 .fi
 .RE
 .PP
@@ -373,7 +373,7 @@
 .RS
 
 .nf
-wpa_supplicant -Dnl80211,wext -c/etc/wpa_supplicant.conf -iwlan0
+wpa_supplicant -Dnl80211,wext -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0
 .fi
 .RE
 .PP
@@ -465,7 +465,7 @@
 .SH "QUICK START"
 .PP
 First, make a configuration file, e.g.
-\fI/etc/wpa_supplicant.conf\fR, that describes the networks
+\fI@TERMUX_PREFIX@/etc/wpa_supplicant.conf\fR, that describes the networks
 you are interested in.  See \fBwpa_supplicant.conf\fR(5)
 for details.
 .PP
@@ -477,7 +477,7 @@
 .RS
 
 .nf
-wpa_supplicant -iwlan0 -c/etc/wpa_supplicant.conf -d
+wpa_supplicant -iwlan0 -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -d
     
 .fi
 .RE
@@ -489,7 +489,7 @@
 .RS
 
 .nf
-wpa_supplicant -iwlan0 -c/etc/wpa_supplicant.conf -B
+wpa_supplicant -iwlan0 -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -B
     
 .fi
 .RE
@@ -504,16 +504,16 @@
 can be used to enable WPA support:
 .PP
 Add MODE="Managed" and WPA="y" to the network scheme in
-\fI/etc/pcmcia/wireless.opts\fR\&.
+\fI@TERMUX_PREFIX@/etc/pcmcia/wireless.opts\fR\&.
 .PP
 Add the following block to the end of \fBstart\fR
-action handler in \fI/etc/pcmcia/wireless\fR:
+action handler in \fI@TERMUX_PREFIX@/etc/pcmcia/wireless\fR:
 .sp
 .RS
 
 .nf
-if [ "$WPA" = "y" -a -x /usr/local/bin/wpa_supplicant ]; then
-    /usr/local/bin/wpa_supplicant -B -c/etc/wpa_supplicant.conf -i$DEVICE
+if [ "$WPA" = "y" -a -x @TERMUX_PREFIX@/bin/wpa_supplicant ]; then
+    @TERMUX_PREFIX@/bin/wpa_supplicant -B -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -i$DEVICE
 fi
     
 .fi
@@ -521,12 +521,12 @@
 .PP
 Add the following block to the end of \fBstop\fR
 action handler (may need to be separated from other actions) in
-\fI/etc/pcmcia/wireless\fR:
+\fI@TERMUX_PREFIX@/etc/pcmcia/wireless\fR:
 .sp
 .RS
 
 .nf
-if [ "$WPA" = "y" -a -x /usr/local/bin/wpa_supplicant ]; then
+if [ "$WPA" = "y" -a -x @TERMUX_PREFIX@/bin/wpa_supplicant ]; then
     killall wpa_supplicant
 fi
     
diff -u -r ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.conf.5 ./wpa_supplicant/doc/docbook/wpa_supplicant.conf.5
--- ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.conf.5	2020-03-10 21:49:08.458858646 +0100
+++ ./wpa_supplicant/doc/docbook/wpa_supplicant.conf.5	2020-03-10 21:52:22.882996517 +0100
@@ -12,7 +12,7 @@
 \fBwpa_supplicant\fR is configured using a text
 file that lists all accepted networks and security policies,
 including pre-shared keys. See the example configuration file,
-probably in \fB/usr/share/doc/wpa_supplicant/\fR, for
+probably in \fB@TERMUX_PREFIX@/share/doc/wpa_supplicant/\fR, for
 detailed information about the configuration format and supported
 fields.
 .PP
@@ -60,9 +60,9 @@
 	group=CCMP TKIP
 	eap=TLS
 	identity="user@example.com"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 }
 .fi
@@ -84,7 +84,7 @@
 	eap=PEAP
 	identity="user@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
 	phase1="peaplabel=0"
 	phase2="auth=MSCHAPV2"
 }
@@ -108,7 +108,7 @@
 	identity="user@example.com"
 	anonymous_identity="anonymous@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
 	phase2="auth=MD5"
 }
 .fi
@@ -129,9 +129,9 @@
 	key_mgmt=IEEE8021X
 	eap=TLS
 	identity="user@example.com"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 	eapol_flags=3
 }
@@ -159,14 +159,14 @@
 	eap=TTLS PEAP TLS
 	identity="user@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 	phase1="peaplabel=0"
-	ca_cert2="/etc/cert/ca2.pem"
-	client_cert2="/etc/cer/user.pem"
-	private_key2="/etc/cer/user.prv"
+	ca_cert2="@TERMUX_PREFIX@/etc/cert/ca2.pem"
+	client_cert2="@TERMUX_PREFIX@/etc/cer/user.pem"
+	private_key2="@TERMUX_PREFIX@/etc/cer/user.prv"
 	private_key2_passwd="password"
 }
 .fi
diff -u -r ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.conf.sgml ./wpa_supplicant/doc/docbook/wpa_supplicant.conf.sgml
--- ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.conf.sgml	2020-03-10 21:49:08.458858646 +0100
+++ ./wpa_supplicant/doc/docbook/wpa_supplicant.conf.sgml	2020-03-10 21:52:22.876333136 +0100
@@ -14,7 +14,7 @@
     <para><command>wpa_supplicant</command> is configured using a text
     file that lists all accepted networks and security policies,
     including pre-shared keys. See the example configuration file,
-    probably in <command>/usr/share/doc/wpa_supplicant/</command>, for
+    probably in <command>@TERMUX_PREFIX@/share/doc/wpa_supplicant/</command>, for
     detailed information about the configuration format and supported
     fields.</para>
 
@@ -65,9 +65,9 @@
 	group=CCMP TKIP
 	eap=TLS
 	identity="user@example.com"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 }
 </programlisting></blockquote>   
@@ -87,7 +87,7 @@
 	eap=PEAP
 	identity="user@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
 	phase1="peaplabel=0"
 	phase2="auth=MSCHAPV2"
 }
@@ -110,7 +110,7 @@
 	identity="user@example.com"
 	anonymous_identity="anonymous@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
 	phase2="auth=MD5"
 }
 </programlisting></blockquote>
@@ -130,9 +130,9 @@
 	key_mgmt=IEEE8021X
 	eap=TLS
 	identity="user@example.com"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 	eapol_flags=3
 }
@@ -159,14 +159,14 @@
 	eap=TTLS PEAP TLS
 	identity="user@example.com"
 	password="foobar"
-	ca_cert="/etc/cert/ca.pem"
-	client_cert="/etc/cert/user.pem"
-	private_key="/etc/cert/user.prv"
+	ca_cert="@TERMUX_PREFIX@/etc/cert/ca.pem"
+	client_cert="@TERMUX_PREFIX@/etc/cert/user.pem"
+	private_key="@TERMUX_PREFIX@/etc/cert/user.prv"
 	private_key_passwd="password"
 	phase1="peaplabel=0"
-	ca_cert2="/etc/cert/ca2.pem"
-	client_cert2="/etc/cer/user.pem"
-	private_key2="/etc/cer/user.prv"
+	ca_cert2="@TERMUX_PREFIX@/etc/cert/ca2.pem"
+	client_cert2="@TERMUX_PREFIX@/etc/cer/user.pem"
+	private_key2="@TERMUX_PREFIX@/etc/cer/user.prv"
 	private_key2_passwd="password"
 }
 </programlisting></blockquote>
diff -u -r ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.sgml ./wpa_supplicant/doc/docbook/wpa_supplicant.sgml
--- ../wpa_supplicant-doc.orig/docbook/wpa_supplicant.sgml	2020-03-10 21:49:08.458858646 +0100
+++ ./wpa_supplicant/doc/docbook/wpa_supplicant.sgml	2020-03-10 21:52:22.873001446 +0100
@@ -505,7 +505,7 @@
     started with:</para>
 
 <blockquote><programlisting>
-wpa_supplicant -B -c/etc/wpa_supplicant.conf -iwlan0
+wpa_supplicant -B -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0
 </programlisting></blockquote>
 
     <para>This makes the process fork into background.</para>
@@ -515,7 +515,7 @@
     foreground with debugging enabled:</para>
 
 <blockquote><programlisting>
-wpa_supplicant -c/etc/wpa_supplicant.conf -iwlan0 -d
+wpa_supplicant -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0 -d
 </programlisting></blockquote>
 
     <para>If the specific driver wrapper is not known beforehand, it is
@@ -524,7 +524,7 @@
     wrapper that is able to initialize the interface.</para>
 
 <blockquote><programlisting>
-wpa_supplicant -Dnl80211,wext -c/etc/wpa_supplicant.conf -iwlan0
+wpa_supplicant -Dnl80211,wext -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -iwlan0
 </programlisting></blockquote>
 
     <para><command>wpa_supplicant</command> can control multiple
@@ -657,7 +657,7 @@
     <title>Quick Start</title>
 
     <para>First, make a configuration file, e.g.
-    <filename>/etc/wpa_supplicant.conf</filename>, that describes the networks
+    <filename>@TERMUX_PREFIX@/etc/wpa_supplicant.conf</filename>, that describes the networks
     you are interested in.  See <citerefentry>
 	<refentrytitle>wpa_supplicant.conf</refentrytitle>
 	<manvolnum>5</manvolnum>
@@ -670,7 +670,7 @@
     enabled:</para>
 
     <blockquote><programlisting>
-wpa_supplicant -iwlan0 -c/etc/wpa_supplicant.conf -d
+wpa_supplicant -iwlan0 -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -d
     </programlisting></blockquote>
 
     <para>Assuming everything goes fine, you can start using following
@@ -678,7 +678,7 @@
     without debugging:</para>
 
     <blockquote><programlisting>
-wpa_supplicant -iwlan0 -c/etc/wpa_supplicant.conf -B
+wpa_supplicant -iwlan0 -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -B
     </programlisting></blockquote>
 
     <para>Please note that if you included more than one driver
@@ -699,24 +699,24 @@
     can be used to enable WPA support:</para>
 
     <para>Add MODE="Managed" and WPA="y" to the network scheme in
-    <filename>/etc/pcmcia/wireless.opts</filename>.</para>
+    <filename>@TERMUX_PREFIX@/etc/pcmcia/wireless.opts</filename>.</para>
 
     <para>Add the following block to the end of <emphasis>start</emphasis>
-    action handler in <filename>/etc/pcmcia/wireless</filename>:</para>
+    action handler in <filename>@TERMUX_PREFIX@/etc/pcmcia/wireless</filename>:</para>
 
     <blockquote><programlisting>
-if [ "$WPA" = "y" -a -x /usr/local/bin/wpa_supplicant ]; then
-    /usr/local/bin/wpa_supplicant -B -c/etc/wpa_supplicant.conf -i$DEVICE
+if [ "$WPA" = "y" -a -x @TERMUX_PREFIX@/bin/wpa_supplicant ]; then
+    @TERMUX_PREFIX@/bin/wpa_supplicant -B -c@TERMUX_PREFIX@/etc/wpa_supplicant.conf -i$DEVICE
 fi
     </programlisting></blockquote>
 
 
     <para>Add the following block to the end of <emphasis>stop</emphasis>
     action handler (may need to be separated from other actions) in
-    <filename>/etc/pcmcia/wireless</filename>:</para>
+    <filename>@TERMUX_PREFIX@/etc/pcmcia/wireless</filename>:</para>
 
     <blockquote><programlisting>
-if [ "$WPA" = "y" -a -x /usr/local/bin/wpa_supplicant ]; then
+if [ "$WPA" = "y" -a -x @TERMUX_PREFIX@/bin/wpa_supplicant ]; then
     killall wpa_supplicant
 fi
     </programlisting></blockquote>
